**Classless Inter-Domain Routing**

From Wikipedia, the free encyclopedia

[Jump to navigation](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#mw-head) [Jump to search](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#searchInput)

"CIDR" redirects here. For other uses, see [CIDR (disambiguation)](https://en.wikipedia.org/wiki/CIDR_(disambiguation)).

**Classless Inter-Domain Routing** (**CIDR** [/ˈsaɪdər, ˈsɪ-/](https://en.wikipedia.org/wiki/Help:IPA/English)) is a method for allocating [IP addresses](https://en.wikipedia.org/wiki/IP_address) and for [IP routing](https://en.wikipedia.org/wiki/IP_routing). The [Internet Engineering Task Force](https://en.wikipedia.org/wiki/Internet_Engineering_Task_Force) introduced CIDR in 1993 to replace the previous [classful network](https://en.wikipedia.org/wiki/Classful_network) addressing architecture on the [Internet](https://en.wikipedia.org/wiki/Internet). Its goal was to slow the growth of [routing tables](https://en.wikipedia.org/wiki/Routing_table) on [routers](https://en.wikipedia.org/wiki/Router_(computing)) across the Internet, and to help slow the rapid [exhaustion of IPv4 addresses](https://en.wikipedia.org/wiki/IPv4_address_exhaustion).[[1]](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#cite_note-RFC_1518-1)[[2]](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#cite_note-RFC_1519-2)

IP addresses are described as consisting of two groups of [bits](https://en.wikipedia.org/wiki/Bit) in the address: the [most significant bits](https://en.wikipedia.org/wiki/Most_significant_bit) are the [network prefix](https://en.wikipedia.org/wiki/Network_prefix), which identifies a whole network or [subnet](https://en.wikipedia.org/wiki/Subnetwork), and the [least significant](https://en.wikipedia.org/wiki/Least_significant_bit) set forms the *host identifier*, which specifies a particular interface of a host on that network. This division is used as the basis of traffic routing between IP networks and for address allocation policies.

Whereas classful network design for [IPv4](https://en.wikipedia.org/wiki/IPv4) sized the network prefix as one or more 8-bit groups, resulting in the blocks of Class A, B, or C addresses, under CIDR address space is allocated to [Internet service providers](https://en.wikipedia.org/wiki/Internet_service_provider) and [end users](https://en.wikipedia.org/wiki/End_user) on any address-bit boundary. In [IPv6](https://en.wikipedia.org/wiki/IPv6), however, the interface identifier has a fixed size of 64 bits by convention, and smaller subnets are never allocated to end users.

CIDR encompasses several concepts. It is based on **variable-length subnet masking** (**VLSM**) which allows the specification of arbitrary-length prefixes. CIDR introduced a new method of representation for IP addresses, now commonly known as **CIDR notation**, in which an address or routing prefix is written with a suffix indicating the number of bits of the prefix, such as *192.0.2.0/24* for IPv4, and *2001:db8::/32* for IPv6. CIDR introduced an administrative process of allocating address blocks to organizations based on their actual and short-term projected needs. The aggregation of multiple contiguous prefixes resulted in [supernets](https://en.wikipedia.org/wiki/Supernet) in the larger Internet, which whenever possible are advertised as aggregates, thus reducing the number of entries in the global routing table.



**Contents**

* [1 Background](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#Background)
* [2 CIDR notation](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#CIDR_notation)
* [3 Subnet masks](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#Subnet_masks)
* [4 CIDR blocks](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#CIDR_blocks)
  + [4.1 Assignment of CIDR blocks](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#Assignment_of_CIDR_blocks)
  + [4.2 IPv4 CIDR blocks](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#IPv4_CIDR_blocks)
  + [4.3 IPv6 CIDR blocks](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#IPv6_CIDR_blocks)
* [5 Prefix aggregation](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#Prefix_aggregation)
* [6 See also](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#See_also)
* [7 References](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#References)
* [8 Further reading](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#Further_reading)
* [9 External links](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#External_links)

**Background**

An IP address is interpreted as composed of two parts: a network-identifying prefix followed by a [host](https://en.wikipedia.org/wiki/Host_(network)) identifier within that network. In the previous [classful network](https://en.wikipedia.org/wiki/Classful_network) architecture, IP address allocations were based on the bit boundaries of the four [octets](https://en.wikipedia.org/wiki/Octet_(computing)) of an IP address. An address was considered to be the combination of an 8, 16, or 24-bit network prefix along with a 24, 16, or 8-bit host identifier respectively. Thus, the smallest allocation and routing block contained only 256 addresses—too small for most enterprises, and the next larger block contained 65536 addresses—too large to be used efficiently even by large organizations. This led to inefficiencies in address use as well as inefficiencies in routing, because it required a large number of allocated class-C networks with individual route announcements, being geographically dispersed with little opportunity for [route aggregation](https://en.wikipedia.org/wiki/Route_aggregation).

During the first decade of the Internet after the invention of the [Domain Name System](https://en.wikipedia.org/wiki/Domain_Name_System) (DNS) it became apparent that the devised system based on the classful network scheme of allocating the IP address space and the routing of IP packets was not [scalable](https://en.wikipedia.org/wiki/Scalability).[[3]](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#cite_note-RFC_1517-3) This led to the successive development of [subnetting](https://en.wikipedia.org/wiki/Subnetwork) and CIDR. The network class distinctions were removed, and the new system was described as being *classless*, with respect to the old system, which became known as *classful*. In 1993, the [Internet Engineering Task Force](https://en.wikipedia.org/wiki/Internet_Engineering_Task_Force) published a new set of standards, [RFC](https://en.wikipedia.org/wiki/RFC_(identifier)) [1518](https://tools.ietf.org/html/rfc1518) and [RFC](https://en.wikipedia.org/wiki/RFC_(identifier)) [1519](https://tools.ietf.org/html/rfc1519), to define this new concept of allocation of IP address blocks and new methods of routing IPv4 packets. An updated version of the specification was published as [RFC](https://en.wikipedia.org/wiki/RFC_(identifier)) [4632](https://tools.ietf.org/html/rfc4632) in 2006.[[4]](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#cite_note-RFC_4632-4)

Classless Inter-Domain Routing is based on variable-length subnet masking (VLSM), which allows a network to be divided into variously sized subnets, providing the opportunity to size a network more appropriately for local needs. Variable-length subnet masks are mentioned in [RFC](https://en.wikipedia.org/wiki/RFC_(identifier)) [950](https://tools.ietf.org/html/rfc950).[[5]](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#cite_note-RFC_950_2.1-5) Accordingly, techniques for grouping addresses for common operations were based on the concept of cluster addressing, first proposed by Carl-Herbert Rokitansky.[[6]](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#cite_note-6)[[7]](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#cite_note-7)

**CIDR notation**

CIDR notation is a compact representation of an IP address and its associated routing prefix. The notation is constructed from an IP address, a [slash](https://en.wikipedia.org/wiki/Slash_(punctuation)) ('/') character, and a decimal number. The trailing number is the count of leading *1* bits in the routing mask, traditionally called the network mask. The IP address in the notation is always represented according to the standards for IPv4 or IPv6.

The address may denote a single, distinct interface address, or it may be the beginning address of an entire network. When expressing a network, its size is given by the number of addresses that are possible with the number of remaining, least-significant bits below the prefix, i.e. the host identifier.

For example:

* *192.168.100.14/24* represents the IPv4 address *192.168.100.14* and its associated routing prefix *192.168.100.0*, or equivalently, its subnet mask *255.255.255.0*, which has 24 leading 1-bits.
* the IPv4 block *192.168.100.0/22* represents the 1024 IPv4 addresses from *192.168.100.0* to *192.168.103.255*.
* the IPv6 block *2001:db8::/48* represents the block of IPv6 addresses from *2001:db8:0:0:0:0:0:0* to *2001:db8:0:ffff:ffff:ffff:ffff:ffff*.
* *::1/128* represents the IPv6 [loopback](https://en.wikipedia.org/wiki/Loopback) address. Its prefix length is 128 which is the number of bits in the address.


For IPv4, CIDR notation is an alternative to the older system of representing networks by their starting address and the subnet mask, both written in [dot-decimal notation](https://en.wikipedia.org/wiki/Dot-decimal_notation). *192.168.100.0/24* is equivalent to *192.168.100.0/255.255.255.0*.

The number of addresses of a subnet may be calculated as 2address length − prefix length, where *address length* is 128 for IPv6 and 32 for IPv4. For example, in IPv4, the prefix length */29* gives: 232 − 29 = 23 = 8 addresses.

**Subnet masks**

A subnet mask is a [bitmask](https://en.wikipedia.org/wiki/Bitmask) that encodes the prefix length associated with an IPv4 address or network in quad-dotted notation: 32 bits, starting with a number of 1 bits equal to the prefix length, ending with 0 bits, and encoded in four-part dotted-decimal format: *255.255.255.0*. A subnet mask encodes the same information as a prefix length but predates the advent of CIDR. In CIDR notation, the prefix bits are always contiguous. Subnet masks were allowed by [RFC](https://en.wikipedia.org/wiki/RFC_(identifier)) [950](https://tools.ietf.org/html/rfc950)[[5]](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#cite_note-RFC_950_2.1-5) to specify non-contiguous bits until [RFC](https://en.wikipedia.org/wiki/RFC_(identifier)) [4632](https://tools.ietf.org/html/rfc4632)[[4]](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#cite_note-RFC_4632-4):Section 5.1 stated that the mask must be left contiguous. Given this constraint, a subnet mask and CIDR notation serve exactly the same function.

**CIDR blocks**

[](https://en.wikipedia.org/wiki/File:IP_Address_Match.svg)


CIDR is principally a bitwise, prefix-based standard for the representation of IP addresses and their routing properties. It facilitates routing by allowing blocks of addresses to be grouped into single routing table entries. These groups, commonly called CIDR blocks, share an initial sequence of bits in the binary representation of their IP addresses. IPv4 CIDR blocks are identified using a syntax similar to that of IPv4 addresses: a dotted-decimal address, followed by a slash, then a number from 0 to 32, i.e., *a.b.c.d/n*. The dotted decimal portion is the IPv4 address. The number following the slash is the prefix length, the number of shared initial bits, counting from the most-significant bit of the address. When emphasizing only the size of a network, the address portion of the notation is usually omitted. Thus, a /20 block is a CIDR block with an unspecified 20-bit prefix.

An IP address is part of a CIDR block and is said to match the CIDR prefix if the initial *n* bits of the address and the CIDR prefix are the same. An IPv4 address is 32 bits so an *n*-bit CIDR prefix leaves 32 − *n* bits unmatched, meaning that 232 − *n* IPv4 addresses match a given *n*-bit CIDR prefix. Shorter CIDR prefixes match more addresses, while longer prefixes match fewer. In the case of overlaid CIDR blocks, an address can match multiple CIDR prefixes of different lengths.

CIDR is also used for [IPv6 addresses](https://en.wikipedia.org/wiki/IPv6_address) and the syntax semantic is identical. The prefix length can range from 0 to 128, due to the larger number of bits in the address. However, by convention, a subnet on broadcast MAC layer networks always has 64-bit host identifiers. Larger prefixes are rarely used even on point-to-point links.[[*citation needed*](https://en.wikipedia.org/wiki/Wikipedia:Citation_needed)]

**Assignment of CIDR blocks**

The [Internet Assigned Numbers Authority](https://en.wikipedia.org/wiki/Internet_Assigned_Numbers_Authority) (IANA) issues to [regional Internet registries](https://en.wikipedia.org/wiki/Regional_Internet_registry) (RIRs) large, short-prefix CIDR blocks. For example, *62.0.0.0/8* (with over sixteen million addresses) is administered by [RIPE NCC](https://en.wikipedia.org/wiki/RIPE_NCC), the European RIR. The RIRs, each responsible for a single, large, geographic area, such as Europe or North America, subdivide these blocks and allocate subnets to local Internet registries (LIRs). Similar subdividing may be repeated several times at lower levels of delegation. End-user networks receive subnets sized according to their projected short-term need. Networks served by a single ISP are encouraged by [IETF](https://en.wikipedia.org/wiki/IETF) recommendations to obtain IP address space directly from their ISP. Networks served by multiple ISPs, on the other hand, may obtain [provider-independent address space](https://en.wikipedia.org/wiki/Provider-independent_address_space) directly from the appropriate RIR.

[](https://en.wikipedia.org/wiki/File:CIDR_Address.svg)

For example, in the late 1990s, the IP address *208.130.29.33* (since reassigned) was used by www.freesoft.org. An analysis of this address identified three CIDR prefixes. *208.128.0.0/11*, a large CIDR block containing over 2 million addresses, had been assigned by [ARIN](https://en.wikipedia.org/wiki/American_Registry_for_Internet_Numbers) (the North American RIR) to [MCI](https://en.wikipedia.org/wiki/MCI_Communications). Automation Research Systems, a Virginia VAR, leased an Internet connection from MCI and was assigned the *208.130.28.0/22* block, capable of addressing just over 1000 devices. ARS used a */24* block for its publicly accessible servers, of which *208.130.29.33* was one. All of these CIDR prefixes would be used, at different locations in the network. Outside MCI's network, the *208.128.0.0/11* prefix would be used to direct to MCI traffic bound not only for *208.130.29.33*, but also for any of the roughly two million IP addresses with the same initial 11 bits. Within MCI's network, *208.130.28.0/22* would become visible, directing traffic to the leased line serving ARS. Only within the ARS corporate network would the *208.130.29.0/24* prefix have been used.


**IPv4 CIDR blocks**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| IPv4 CIDR | | | | | | | |
| **Address format** | **Difference to last address** | **Mask** | **Addresses** | | **Relative to class A, B, C** | **Restrictions on *a*, *b*, *c* and *d* (0..255 unless noted)** | **Typical use** |
| **Decimal** | **2*n*** |
| *a.b.c.d/32* | +*0.0.0.0* | *255.255.255.255* | 1 | 20 | ​1⁄256 C |  | Host route |
| *a.b.c.d/31* | +*0.0.0.1* | *255.255.255.254* | 2 | 21 | ​1⁄128 C | *d* = 0 ... (2*n*) ... 254 | Point-to-point links ([RFC](https://en.wikipedia.org/wiki/RFC_(identifier)) [3021](https://tools.ietf.org/html/rfc3021)) |
| *a.b.c.d/30* | +*0.0.0.3* | *255.255.255.252* | 4 | 22 | ​1⁄64 C | *d* = 0 ... (4*n*) ... 252 | Point-to-point links (glue network) |
| *a.b.c.d/29* | +*0.0.0.7* | *255.255.255.248* | 8 | 23 | ​1⁄32 C | *d* = 0 ... (8*n*) ... 248 | Smallest multi-host network |
| *a.b.c.d/28* | +*0.0.0.15* | *255.255.255.240* | 16 | 24 | ​1⁄16 C | *d* = 0 ... (16*n*) ... 240 | Small [LAN](https://en.wikipedia.org/wiki/LAN) |
| *a.b.c.d/27* | +*0.0.0.31* | *255.255.255.224* | 32 | 25 | ⅛ C | *d* = 0 ... (32*n*) ... 224 |
| *a.b.c.d/26* | +*0.0.0.63* | *255.255.255.192* | 64 | 26 | ¼ C | *d* = 0, 64, 128, 192 |
| *a.b.c.d/25* | +*0.0.0.127* | *255.255.255.128* | 128 | 27 | ½ C | *d* = 0, 128 | Large [LAN](https://en.wikipedia.org/wiki/LAN) |
| *a.b.c.0/24* | +*0.0.0.255* | *255.255.255.0* | 256 | 28 | 1 C |  |
| *a.b.c.0/23* | +*0.0.1.255* | *255.255.254.0* | 512 | 29 | 2 C | *c* = 0 ... (2*n*) ... 254 |  |
| *a.b.c.0/22* | +*0.0.3.255* | *255.255.252.0* | 1,024 | 210 | 4 C | *c* = 0 ... (4*n*) ... 252 | Small business |
| *a.b.c.0/21* | +*0.0.7.255* | *255.255.248.0* | 2,048 | 211 | 8 C | *c* = 0 ... (8*n*) ... 248 | Small [ISP](https://en.wikipedia.org/wiki/ISP)/ large business |
| *a.b.c.0/20* | +*0.0.15.255* | *255.255.240.0* | 4,096 | 212 | 16 C | *c* = 0 ... (16*n*) ... 240 |
| *a.b.c.0/19* | +*0.0.31.255* | *255.255.224.0* | 8,192 | 213 | 32 C | *c* = 0 ... (32*n*) ... 224 | [ISP](https://en.wikipedia.org/wiki/ISP)/ large business |
| *a.b.c.0/18* | +*0.0.63.255* | *255.255.192.0* | 16,384 | 214 | 64 C | *c* = 0, 64, 128, 192 |
| *a.b.c.0/17* | +*0.0.127.255* | *255.255.128.0* | 32,768 | 215 | 128 C | *c* = 0, 128 |
| *a.b.0.0/16* | +*0.0.255.255* | *255.255.0.0* | 65,536 | 216 | 256 C = B |  |  |
| *a.b.0.0/15* | +*0.1.255.255* | *255.254.0.0* | 131,072 | 217 | 2 B | *b* = 0 ... (2*n*) ... 254 |  |
| *a.b.0.0/14* | +*0.3.255.255* | *255.252.0.0* | 262,144 | 218 | 4 B | *b* = 0 ... (4*n*) ... 252 |  |
| *a.b.0.0/13* | +*0.7.255.255* | *255.248.0.0* | 524,288 | 219 | 8 B | *b* = 0 ... (8*n*) ... 248 |  |
| *a.b.0.0/12* | +*0.15.255.255* | *255.240.0.0* | 1,048,576 | 220 | 16 B | *b* = 0 ... (16*n*) ... 240 |  |
| *a.b.0.0/11* | +*0.31.255.255* | *255.224.0.0* | 2,097,152 | 221 | 32 B | *b* = 0 ... (32*n*) ... 224 |  |
| *a.b.0.0/10* | +*0.63.255.255* | *255.192.0.0* | 4,194,304 | 222 | 64 B | *b* = 0, 64, 128, 192 |  |
| *a.b.0.0/9* | +*0.127.255.255* | *255.128.0.0* | 8,388,608 | 223 | 128 B | *b* = 0, 128 |  |
| *a.0.0.0/8* | +*0.255.255.255* | *255.0.0.0* | 16,777,216 | 224 | 256 B = A |  | Largest [IANA](https://en.wikipedia.org/wiki/Internet_Assigned_Numbers_Authority) block allocation |
| *a.0.0.0/7* | +*1.255.255.255* | *254.0.0.0* | 33,554,432 | 225 | 2 A | *a* = 0 ... (2*n*) ... 254 |  |
| *a.0.0.0/6* | +*3.255.255.255* | *252.0.0.0* | 67,108,864 | 226 | 4 A | *a* = 0 ... (4*n*) ... 252 |  |
| *a.0.0.0/5* | +*7.255.255.255* | *248.0.0.0* | 134,217,728 | 227 | 8 A | *a* = 0 ... (8*n*) ... 248 |  |
| *a.0.0.0/4* | +*15.255.255.255* | *240.0.0.0* | 268,435,456 | 228 | 16 A | *a* = 0 ... (16*n*) ... 240 |  |
| *a.0.0.0/3* | +*31.255.255.255* | *224.0.0.0* | 536,870,912 | 229 | 32 A | *a* = 0 ... (32*n*) ... 224 |  |
| *a.0.0.0/2* | +*63.255.255.255* | *192.0.0.0* | 1,073,741,824 | 230 | 64 A | *a* = 0, 64, 128, 192 |  |
| *a.0.0.0/1* | +*127.255.255.255* | *128.0.0.0* | 2,147,483,648 | 231 | 128 A | *a* = 0, 128 |  |
| *0.0.0.0/0* | +*255.255.255.255* | *0.0.0.0* | 4,294,967,296 | 232 | 256 A |  |  |

In common usage, the first address in a subnet, all binary zero in the host identifier, is reserved for referring to the network itself, while the last address, all binary one in the host identifier, is used as a [broadcast address](https://en.wikipedia.org/wiki/Broadcast_address) for the network; this reduces the number of addresses available for hosts by 2. As a result, a */31* network, with one binary digit in the host identifier, would be unusable, as such a subnet would provide no available host addresses after this reduction. [RFC](https://en.wikipedia.org/wiki/RFC_(identifier)) [3021](https://tools.ietf.org/html/rfc3021) creates an exception to the "host all ones" and "host all zeros" rules to make */31* networks usable for point-to-point links. */32* addresses (single-host network) must be accessed by explicit routing rules, as there is no room in such a network for a gateway.

In routed subnets larger than */31* or */32*, the number of available host addresses is usually reduced by two, namely the largest address, which is reserved as the broadcast address, and the smallest address, which identifies the network itself.[[8]](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#cite_note-RFC_922-8)[[9]](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#cite_note-RFC_1812-9)

**IPv6 CIDR blocks**

[](https://en.wikipedia.org/wiki/File:IPv6_CIDR_table-en.svg)

A Table of CIDR prefixes for IPv6, it shows the number of corresponding equivalent subnets for each prefix, as well as the number of the host identifier bits.

The large address size used in IPv6 permitted implementation of worldwide route summarization and guaranteed sufficient address pools at each site. The standard subnet size for IPv6 networks is a */64* block, which is required for the operation of [stateless address autoconfiguration](https://en.wikipedia.org/wiki/IPv6_stateless_address_autoconfiguration).[[10]](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#cite_note-RFC_4862-10) At first, the IETF recommended in [RFC](https://en.wikipedia.org/wiki/RFC_(identifier)) [3177](https://tools.ietf.org/html/rfc3177) as a best practice that all end sites receive a */48* address allocation,[[11]](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#cite_note-RFC_3177-11) however, criticism and reevaluation of actual needs and practices has led to more flexible allocation recommendations in [RFC](https://en.wikipedia.org/wiki/RFC_(identifier)) [6177](https://tools.ietf.org/html/rfc6177)[[12]](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#cite_note-RFC_6177-12) suggesting a significantly smaller allocation for some sites, such as a */56* block for home networks.

This **IPv6 subnetting reference** lists the sizes for IPv6 [subnetworks](https://en.wikipedia.org/wiki/Subnetwork). Different types of network links may require different subnet sizes.[[13]](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#cite_note-13) The subnet mask separates the bits of the network identifier prefix from the bits of the interface identifier. Selecting a smaller prefix size results in fewer number of networks covered, but with more addresses within each network.[[14]](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#cite_note-14)

2001:0db8:0123:4567:89ab:cdef:1234:5678

|||| |||| |||| |||| |||| |||| |||| ||||

|||| |||| |||| |||| |||| |||| |||| |||128 Single end-points and [loopback](https://en.wikipedia.org/wiki/Loopback)

|||| |||| |||| |||| |||| |||| |||| |||127 Point-to-point links (inter-router)

|||| |||| |||| |||| |||| |||| |||| ||124

|||| |||| |||| |||| |||| |||| |||| |120

|||| |||| |||| |||| |||| |||| |||| 116

|||| |||| |||| |||| |||| |||| |||112

|||| |||| |||| |||| |||| |||| ||108

|||| |||| |||| |||| |||| |||| |104

|||| |||| |||| |||| |||| |||| 100

|||| |||| |||| |||| |||| |||96

|||| |||| |||| |||| |||| ||92

|||| |||| |||| |||| |||| |88

|||| |||| |||| |||| |||| 84

|||| |||| |||| |||| |||80

|||| |||| |||| |||| ||76

|||| |||| |||| |||| |72

|||| |||| |||| |||| 68

|||| |||| |||| |||64 Single LAN; default prefix size for [SLAAC](https://en.wikipedia.org/wiki/SLAAC)

|||| |||| |||| ||60 Some (very limited) [6rd](https://en.wikipedia.org/wiki/6rd) deployments (/60 = 16 /64 blocks)

|||| |||| |||| |56 Minimal end sites assignment[[12]](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#cite_note-RFC_6177-12); e.g. [home network](https://en.wikipedia.org/wiki/Home_network) (/56 = 256 /64 blocks)

|||| |||| |||| 52 /52 block = 4096 /64 blocks

|||| |||| |||48 Typical assignment for larger sites (/48 = 65536 /64 blocks)

|||| |||| ||44

|||| |||| |40

|||| |||| 36 possible future [local Internet registry](https://en.wikipedia.org/wiki/Local_Internet_registry) (LIR) extra-small allocations

|||| |||32 LIR minimum allocations

|||| ||28 LIR medium allocations

|||| |24 LIR large allocations

|||| 20 LIR extra large allocations

|||16

||12 [Regional Internet registry](https://en.wikipedia.org/wiki/Regional_Internet_registry) (RIR) allocations from IANA[[15]](https://en.wikipedia.org/wiki/Classless_Inter-Domain_Routing#cite_note-15)

|8

4

**Prefix aggregation**

CIDR provides fine-grained [routing prefix aggregation](https://en.wikipedia.org/wiki/Routing_prefix_aggregation). For example, if the first 20 bits of their network prefixes match, sixteen contiguous /24 networks can be aggregated and advertised to a larger network as a single /20 [routing table](https://en.wikipedia.org/wiki/Routing_table) entry. This reduces the number of routes that have to be advertised.

**See also**

* [Internet protocol suite](https://en.wikipedia.org/wiki/Internet_protocol_suite)

**References**

 *Y. Rekhter; T. Li (September 1993).* [*An Architecture for IP Address Allocation with CIDR*](https://tools.ietf.org/html/rfc1518)*.* [*doi*](https://en.wikipedia.org/wiki/Doi_(identifier))*:*[*10.17487/RFC1518*](https://doi.org/10.17487%2FRFC1518)*.* [*RFC*](https://en.wikipedia.org/wiki/RFC_(identifier))[*1518*](https://tools.ietf.org/html/rfc1518)*.*

  *V. Fuller; T. Li; J. Yu; K. Varadhan (September 1993).* [*Classless Inter-Domain Routing (CIDR): an Address Assignment and Aggregation Strategy*](https://tools.ietf.org/html/rfc1519)*.* [*doi*](https://en.wikipedia.org/wiki/Doi_(identifier))*:*[*10.17487/RFC1519*](https://doi.org/10.17487%2FRFC1519)*.* [*RFC*](https://en.wikipedia.org/wiki/RFC_(identifier))[*1519*](https://tools.ietf.org/html/rfc1519)*.*

  *R. Hinden, ed. (September 1993).* [*Applicability Statement for the Implementation of Classless Inter-Domain Routing (CIDR)*](https://tools.ietf.org/html/rfc1517)*.* [*doi*](https://en.wikipedia.org/wiki/Doi_(identifier))*:*[*10.17487/RFC1517*](https://doi.org/10.17487%2FRFC1517)*.* [*RFC*](https://en.wikipedia.org/wiki/RFC_(identifier))[*1517*](https://tools.ietf.org/html/rfc1517)*.*

  *V. Fuller; T. Li (August 2006).* [*Classless Inter-domain Routing (CIDR): The Internet Address Assignment and Aggregation Plan*](https://tools.ietf.org/html/rfc4632)*.* [*doi*](https://en.wikipedia.org/wiki/Doi_(identifier))*:*[*10.17487/RFC4632*](https://doi.org/10.17487%2FRFC4632)*.* [*RFC*](https://en.wikipedia.org/wiki/RFC_(identifier))[*4632*](https://tools.ietf.org/html/rfc4632)*.*

  *J. Mogul; J. Postel, eds. (August 1985).* [*Internet Standard Subnetting Procedure*](https://tools.ietf.org/html/rfc950#section-2.1)*. sec. 2.1.* [*doi*](https://en.wikipedia.org/wiki/Doi_(identifier))*:*[*10.17487/RFC0950*](https://doi.org/10.17487%2FRFC0950)*.* [*RFC*](https://en.wikipedia.org/wiki/RFC_(identifier))[*950*](https://tools.ietf.org/html/rfc950)*.*

  Carl-Herbert Rokitansky, "Internet Cluster Addressing Scheme and its Application to Public Data Networks", Proc. 9th International Conference on Computer Communication (ICCC' 88), pp. 482-491, Tel Aviv, Israel, Oct./Nov. 1988

  [Cluster Addressing and CIDR](http://www.ietf.org/mail-archive/web/ietf/current/msg24136.html) in the mail archives of the IETF

  *J. Mogul, ed. (October 1984).* [*Broadcasting Internet Datagrams in the Presence of Subnets*](https://tools.ietf.org/html/rfc922#section-7)*. sec. 7.* [*doi*](https://en.wikipedia.org/wiki/Doi_(identifier))*:*[*10.17487/RFC0922*](https://doi.org/10.17487%2FRFC0922)*.* [*RFC*](https://en.wikipedia.org/wiki/RFC_(identifier))[*922*](https://tools.ietf.org/html/rfc922)*.*

  *F. Baker, ed. (June 1995).* [*Requirements for IP Version 4 Routers*](https://tools.ietf.org/html/rfc1812#section-4.2.3.1)*. sec. 4.2.3.1.* [*doi*](https://en.wikipedia.org/wiki/Doi_(identifier))*:*[*10.17487/RFC1812*](https://doi.org/10.17487%2FRFC1812)*.* [*RFC*](https://en.wikipedia.org/wiki/RFC_(identifier))[*1812*](https://tools.ietf.org/html/rfc1812)*.*

  [RFC](https://en.wikipedia.org/wiki/RFC_(identifier)) [4862](https://tools.ietf.org/html/rfc4862)

  [*IAB/IESG Recommendation on IPv6 Address Allocations to Sites*](https://tools.ietf.org/html/rfc3177)*. IAB/IESG. September 2001.* [*doi*](https://en.wikipedia.org/wiki/Doi_(identifier))*:*[*10.17487/RFC3177*](https://doi.org/10.17487%2FRFC3177)*.* [*RFC*](https://en.wikipedia.org/wiki/RFC_(identifier))[*3177*](https://tools.ietf.org/html/rfc3177)*.*

  *T. Narten; G. Huston; L. Roberts (March 2011).* [*IPv6 Address Assignment to End Sites*](https://tools.ietf.org/html/rfc6177)*.* [*doi*](https://en.wikipedia.org/wiki/Doi_(identifier))*:*[*10.17487/RFC6177*](https://doi.org/10.17487%2FRFC6177)*.* [*RFC*](https://en.wikipedia.org/wiki/RFC_(identifier))[*6177*](https://tools.ietf.org/html/rfc6177)*.*

  [*"ARIN IPv6 Addressing Plans"*](http://www.getipv6.info/index.php/IPv6_Addressing_Plans)*. Getipv6.info. 2016-03-25. Retrieved 2018-03-12.*

  [*"RIPE IP Allocation Rates"*](https://web.archive.org/web/20110203130851/http:/ripe.net/info/info-services/addressing.html)*. Archived from* [*the original*](https://www.ripe.net/info/info-services/addressing.html) *on 2011-02-03.*

* 1.  [*"IANA IPv6 unicast address assignments"*](http://www.iana.org/assignments/ipv6-unicast-address-assignments/ipv6-unicast-address-assignments.xml)*. Iana.org. Retrieved 2018-03-12.*

**Further reading**

* [*Classless IN-ADDR.ARPA delegation*](https://tools.ietf.org/html/rfc2317)*. March 1998.* [*doi*](https://en.wikipedia.org/wiki/Doi_(identifier))*:*[*10.17487/RFC2317*](https://doi.org/10.17487%2FRFC2317)*.* [*RFC*](https://en.wikipedia.org/wiki/RFC_(identifier))[*2317*](https://tools.ietf.org/html/rfc2317)*.*
* [*CIDR and Classful Routing*](https://tools.ietf.org/html/rfc1817)*. August 1995.* [*doi*](https://en.wikipedia.org/wiki/Doi_(identifier))*:*[*10.17487/RFC1817*](https://doi.org/10.17487%2FRFC1817)*.* [*RFC*](https://en.wikipedia.org/wiki/RFC_(identifier))[*1817*](https://tools.ietf.org/html/rfc1817)*.*

**External links**

* [CIDR Report](https://www.cidr-report.org/as2.0/) (updated daily)